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Introduction

Among the most fundamental needs of engineers in the field of protection and testing of electrical equipment are precise current and voltage injection devices as well as high-accuracy measurement tools. These instruments play a key role in performing tests and evaluating the performance of critical power-system equipment.
In addition, engineers and specialists involved in the manufacturing, maintenance, and servicing of industrial equipment and high-voltage substations require reliable, accurate tools to carry out tests in accordance with international standards. These tests include examinations of equipment such as power transformers, circuit breakers, disconnectors, current transformers (CTs) and voltage transformers (VTs) across various classes, as well as reactors and capacitor banks.
Drawing on the valuable experience and deep technical expertise of its team, Vebko has succeeded in designing and producing devices that integrate multiple capabilities into a single, unified multi-purpose instrument—significantly reducing the size, weight, and number of devices required, and yielding substantial savings in procurement and maintenance costs for industrial and laboratory environments.
Beyond improving accuracy, repeatability, and test speed, these solutions also enhance the safety and efficiency of the testing process. For this reason, Vebko’s modern test systems are an effective and attractive replacement for traditional, fragmented setups.
Given the broad scope of applications for Vebko’s test devices, a set of accessories and auxiliary tools is also available, including various cables, interfaces, terminals, probes, and adapters, enabling the required connections with the highest levels of safety, accuracy, and electrical stability.
These accessories are offered as dedicated kits, allowing specialists to choose the most appropriate configuration according to test type, operating voltage, and the size of the device under test. This modular design increases ease of execution and provides high flexibility in industrial and laboratory settings.
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	Description
	Code
	QTY
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	Test device with 4 voltage sources and 6 current sources.
8 binary/analog inputs.
2 AC/DC analog inputs.
4 binary outputs.
LAN / Wi-Fi / Serial connectivity.
Weight: 12.5 kg.
Dimensions: 39 cm × 41 cm × 19 cm
	AMT1003
	1
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	Test device with 6 voltage sources and 6 current sources.
8 binary/analog inputs.
2 AC/DC analog inputs.
4 binary outputs.
LAN / Wi-Fi / Serial connectivity.
3 network ports.
Convertible current and voltage sources.
Weight: 12.5 kg.
Dimensions: 39 cm × 41 cm × 19 cm
	AMT2050
	1
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	Protective relay tester carry case for safe transport of the device
	AMT1001
	1
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	Test clamp suitable for various power equipment, with 4 current pins and 1 voltage pin
	AMT1016
	8
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	Protective cover for the test clamp
	AMT1028
	8
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	8-core, 4-color, 3-meter cable for easier connection between the device and the relay, rated 300 V and 32 A per core
	AMT1004
	1
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	RJ45 cable for connecting the device and the laptop
	AMT1007
	1
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	Device power cable
Length: 1.5 m
250 V, 10 A
	AMT1006
	1
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	Alligator clips for connecting to pins or screws during equipment tests
	AMT1012
	4
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	7-meter, 8-core cable suitable for equipment testing
	AMT1015
	3
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	Soft carry bag for the device, with compartments for accessories
	AMT1002
	1

	[image: ]
	Box containing 3 non-polar capacitors, 10,000 µF and 60 V
	AMT1019
	1
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	Flexible test lead with plastic insulation for safe use on test terminals
	AMT1011
	4
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	USB Type-B to USB Type-A cable
	AMT1026
	1
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	Flexible test lead with plastic insulation for safe use on test terminals
	AMT1014
	4
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	Black cable ties
	AMT1013
	5
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	3-meter, 4-core two-color cable suitable for relay and equipment testing
	AMT1005
	5
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	RS-232 dongle and protective fuse for the device
	AMT1020
	1
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	Flexible terminal adapters for screw terminals
	AMT1009
	12
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	Terminal adapters for screw terminals
	AMT1010
	12
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	Grounding cable suitable for the device
	AMT1008
	1
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	Infrared optical sensor for meter testing
	AMT1018
	1
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	GPS antenna for syncing multiple devices, length 15 m
	AMT1017
	1
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	Backpack for carrying cables and test clamps
	AMT1023
	1
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	Suitcase cover for the device to protect it during air and intercity transport
	AMT1024
	1
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	Screwdriver for opening the device (if needed)
	AMT1022
	1
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	Black pouch for small equipment and cables
	AMT1025
	1
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	Cable retainer for bundled cables
	AMT1021
	16
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	instrument Base Plate
	C01-AMT1030
	1
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	Circuit breaker test module – CBA105
	C12-AMT1031
	1
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	CT & CVT test module – CTA105
	C13-AMT1033
	1
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	Transformer test module – TRA105
	C11-AMT1032
	1
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	Electronic Relays Tester Module – RTA105
	C30-AMT1047
	1
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	Auto Calibration – CLA105
	C20-AMT1056
	1
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	BI shunt
	C52-AMT1060
	1
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	Clamp Booster 
	C50-AMT1058
	1
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	Rogowski 
	C53-AMT1061
	1
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	Earthing Test Electrode
	C60-AMT1063        
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	Insulation Resistance Measuring
	C40-AMT1051
	1
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	Arc-flash initiator
	C51-AMT1059
	1
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	G6A Relay
	C31-AMT1055
	1
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	P3C8
	C36-AMT1045
	1
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	DP12
	C32-AMT1041
	1
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	P3H34
	C37-AMT1044
	1
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	DP12 Guide
	C33-AMT2020
	1
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	GPS With 50 Meters Cable
	C55-AMT1049
	1
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	Extended Binary
	C56-AMT1065
	1
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	Sample Value
	C70-AMT1066
	1
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	Recloser Test Cable
	C54-AMT1064
	1
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